Sistemas Informáticos (Computer Systems)  
Unit 10. Disk images

short line

Authors: Sergi García, Alfredo Oltra

Updated March 2024

Licencia

**Reconocimiento - No comercial - CompartirIgual** (BY-NC-SA): No se permite un uso comercial de la obra original ni de las posibles obras derivadas, la distribución de las cuales se ha de hacer con una licencia igual a la que regula la obra original.

Nomenclatura

A lo largo de este tema se utilizarán diferentes símbolos para distinguir elementos importantes dentro del contenido. Estos símbolos son:

📖 **Important**

❕ **Attention**

💬 **Interesting**

**INDEX**

[**1. Disk Images**](#_gjdgxs) **3**

[**2. Programs to make/restore images**](#_30j0zll) **4**

[**3. DRBL**](#_1fob9te) **4**

[**3.1 Multicast**](#_3znysh7) **4**

[**3.2 Download**](#_2et92p0) **5**

[**3.3 Creating the disk Image**](#_tyjcwt) **5**

[**3.4 Restoring the image**](#_3dy6vkm) **8**

[**3.5 Clients**](#_1t3h5sf) **10**

[**4. Bibliography**](#_4d34og8) **10**

Unit 10. Disk images

# Disk Images

A disk image is a file that contains the exact copy (bit by bit) of a storage system, usually a hard disk, although it can be another media such as a USB storage, a DVD, etc. Being an exact copy, not only contains all the data, also the exact structure of the device. This includes sectors that are not “visible” to the user, but which are critical to the system, such as the boot sectors or the partition table.

The generated image can be restored on other devices (obviously, provided the available size is greater than or equal to the size of the original device).


Their main uses are:

* Cloning computers with the same technical characteristics. The user sets up a new machine on all products: partitions, operating system(s), drivers, external connections, basic applications, user accounts, permissions, etc. and once done, we make an image that later restores to multiple computers. Examples of use in a computer room, or departments of companies, in which generally the equipment fleet is identical.
* Recovery of a common starting point. Possibly the image created in the previous section can be used to, in case of system error, return to a known and functional point.
* Migrate from a small hard disk to a larger one.

The great problem with this technique is the space occupied by the copies. The fact of copying bit by bit implies that not only data is copied, but also another type of information that is not necessary to back up and that obviously makes the image files very large. An image of an X GB disk will occupy X GB. To minimize this problem, the programs that make images use two options: do not save unused space and use compression mechanisms.

📖 **Important:** It is very important to note that this system, although it could be confused with a backup system, is not. Neither the generation time,nor the restoration time, nor the fact that when retrieving it on the same computer all content is overwritten and that, of course, the data backed up includes elements other than the data and that it is not possible to filter that data by importance make both concepts, although similar, are not the same.

❕ **Attention:** Beside to cloning an entire disk, it is possible to clone a single partition



*Figure 1 - Schema of clone process*

# Programs to make/restore images

There are a lot of programs to help you to create and restore disk images. Some of them can be:

* ***CloneZilla****:* CloneXilla is a free software disaster recovery, disk cloning and deployment solution. Maybe the most famous and used.
* ***Redo Backup and Recovery****:* Similar functionality to *CloneZilla* (in fact, both of them use the same core). *Redo Backup* has a friendly graphic interface that makes very easy to use it.
* ***Win32 Disk Imager****:* Source code tool for Windows Systems. It works only with USB sticks or SD cards.

# DRBL

As discussed earlier, the use of images allows the creation of multiple identical computers in configuration from one.

The procedure to perform such a kind of cloning is to create the image of the source computer and clone one by one all the target computers. Obviously this process is faster than installing and configuring each of them, but possibly a more optimal solution would be to be able to **simultaneously** clone all computers connecting them on the network.


For this kind of use, one of the best solutions is to use *DRBL*.

*DRBL* is a tool (a Linux distribution) that allows to start an operating system, in the network machines, without having to have any software installed locally. With *CloneZilla* (included in *DRBL*) we will be able to clone in multicast mode, as many machines as we want, simultaneously.

## Multicast


When sending any type of information over a network, there are three ways to do this

* **Unicast**: It is defined by a single sender and a single receiver. The server has a separate connection with each client.




*Figure 2 - Unicast*

* **Broadcast**: In this transmission, the signal reaches far and wide and is available to everyone.



*Figure 3 - Broadcast*

* **Multicast**: Similar to broadcast, but in the multicast if the receiver does not want the signal it does not receive it (in broadcast all the computers in the net receive the signal.



*Figure 4 -Multicast*

## Download

The first step is to get and to burn an ISO of DRBL. You can download it from <http://drbl.org/download/>

📖 **Important:** DBRL is a live SO, so you run the computer with it, and you can use it as an Operative System.

📖 **Important:** There are three options amd64 (to 64-bits processors), 686 (to 32-bit processors), and 686-pae (to 32-bit processors but with support for memories larger than 3 GB). You have to download the version depending on the processor of the computer to clone.


After the download, the next step is to burn the ISO image to a CD/DVD (with a burning program like Nero, Burn, Toast, ISO Burner, etc.) or on a USB stick (with UltraISO, Rufus, etc.)

## Creating the disk Image

The first step is to create the image disk. We start from an installation of *LUbuntu*, where we have created a file on the desktop to verify that the image is properly performed and restored

Restart the computer with the burned DVD with DRBL in the DVD reader or, if you use a USB, with the stick connected. If we let the system start up, it will end up starting a live version of DRBL in graphic mode.

❕ **Attention:** To boot from DVD/BD or USB, it is necessary to have this option activated and/or modify the system boot order. These options can be configured from SETUP

**



*Figure 5 -LUbuntu Desktop*



*Figure 6 - DRBL*

Once the GUI has been loaded, do a double-click on “*Clonezilla Live”* to start the program. This program works in text mode. On the first screen (figure 7) we must choose the working mode:

* **From device to device:** the contents of a hard disk will be cloned in another disk
* **From device to image file**: the contents of a hard disk will be copied into a file. This one is the usual option.





*Figure 7 - Available modes Figure 8 - Select image destination*

Then we will have to choose the location where we want to store the backup (figure 8). There are five options, one in local (a hard drive or USB physically connected to the computer) or some kind of space available in the network, space that can be accessed in several ways (*ssh*, *samba*, etc). In our case, we are going to select a *local\_dev*.

❕ **Attention:** You can not save an image of a partition (or a disk) on the same partition (or the same disk). For instance, if you are going to make an image of, “*/dev/sda3”* you can not save it to “*/dev/sda3”*.

Our *local\_dev* is an external hard disk connected by USB. So we have to connect it and wait five or ten seconds for the system can recognize it.





*Figure 9 - Waiting to insert hard disks Figure 10 - List of available hard disks*

In our case, our *local\_dev* device is located as */dev/sdb, My Passport*. The next step is to mount (to connect) the *local\_dev* with *CloneZilla* logically. So we need to select the device */dev/sdb1*.

❕ **Attention:** on Linux, the devices are simulated using files that are in the *dev* directory. There are many types, but in terms of connected elements in the PATA or SATA connectors, the way to number them is: *type + order + partition*. The types are “*hd”* for PATA devices and “*sd”* for SATA devices. The order refers to the port number element in which they are connected. To do this, letters are used by the “a”. The partitions are numbered with numbers, starting with the number “1”. For instance, “sdb1” refers to the first partition in a device connected to the second SATA port.



Besides, *CloneZilla* allows selecting a directory inside that partition (figure 11). In our case, we select an *MV* folder. So, our images will save in the folder MV inside the first partition of the hard disk connected in the second SATA port.

On the next screen (figure 12), select the *Beginner* mode, and on the next one (figure 13) we need to select if we want to save a full disk or only a partition. In this case, we are going to choose “*savedisk”*, to create an image of the full disk.



*Figure 11 - Select mode Figure 12 - Select folder*


In the next screens, you can modify the name of the image file (figure 14) and select the hard disk that is going to be backed up (figure 15).

*Figure 13 - Save disk Figure 14 - Image name*

The last screens refer to checks, either the file system before the copy (figure 16) or the image once it has been created, and the possibility of encrypting the image. If you trust your system, they can be discarded because all these processes slow down the creation of the images.

Once all the options are configured, the *CloneZilla* will ask for confirmation and will start the creation of the image (figure 17).



*Figure 15 - Select hard disk Figure 16 - Disk checks*



If everything is ok after a few minutes (figure 18) we will have on our disk a folder with our image ready to be cloned.

## Restoring the image

Once we have created the image, the next step is to perform the restoration.

The process can be done by starting the DRBL on the computer to clone, connecting the hard disk where the image is stored and launching the *CloneZilla live* but choosing the restore options.


However, we will see how to perform *multicast* restore, so that we can clone multiple computers simultaneously.



*Figure 17 - Are you sure? Figure 18 - Disk image is done*

We need a computer that has the server functions. In general, the computer in which the image is made is usually used. We boot the computer with DRBL in the same way as to create the image, but this time we start *CloneZilla Server*.

The first time, we will be shown information regarding the lack of initial configuration (figure 19), especially of another IP. By simply type “Y” character, it automatically sets up the entire system.





*Figure 19 - Warning about lack of information*

Once the *Clonezilla* configures the server, the first step is the choice of the image, which is done similarly as it is done in the creation process.



We need to allocate the computers that will serve the server (figure 20), It is possible to tell you all or, if not, a range of IPs or MAC addresses. The most common is the first option and, to avoid problems, disconnect from the network computers that do not need to be cloned.

The next step is to tell the server that what we want is to restore (figure 21), specifying whether what we want to restore will be a partition or a disk. In our case, the image created is from a disk, so we will choose the option to restore the disk.



*Figure 20 - Computers to restore Figure 21 - Operation to perform*

Of course, we have to select the name of the image (figure 22) and the name of the hard disk (figure 23) where the image will be cloned.





*Figure 22 - Image name Figure 23 - Hard disk name*

The last steps are related to communication between teams. The first allows us to choose the mode, be it unicast, multicast or broadcast (figure 25). The second defines the way in which the server waits for clients (figure 26).

* ***Clients + timetowait***: will ask us for the number of clients that have to wait or a maximum time, whichever happens first. It is my preferred option, in case some client is locked, it even starts after a while and then fix what failed in that one.
* ***Time to wait*:** wait for seconds to tell you to connect all the clients you want.
* ***Clients to wait*:** wait for a certain number of clients before starting the process.

Once all the features are defined, the server boots, waiting for clients.


❕ **Attention:** It is very important not to close the window in which the server has been configured



*Figure 24 - Restore mode Figure 25 - Restore method*

## Clients

If the clients have enabled network boot in the BIOS, all you have to do is turn on the computer and the whole process will start automatically. In case you do not support this technique, you will have to start each one with the DRBL CD, but entering the option *Network boot via iPXE* (figure 26)



*Figure 15 - Clients booting with DRBL*

# Bibliography

[1] DRBL <https://drbl.org/>

[2] CloneZilla <https://clonezilla.org/>